In the sampling task, you should use this filter specs

InputFilterType = LOW;

InputFS = 8000;

InputStopBandAttenuation = 50;

InputCutOffFrequency = 1500;

InputTransitionBand = 500;